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SOUTH WEST DESIGN AFRICA LIMITED (SWDA)
RAEC 18-TANK ATC/NME TANK CLEANING PROJECT — Contract/Tender No. CW-68582 / CW-515913
LIKELY CHEMICALS REGISTER — MSDS SUMMARY & SHOC CARD
Tank Cleaning Operations — Chemicals Identified in HSE Plan Attachment 1 (JHSA)
	RAEC Capability Assessment Reference
	Item 5.2(e)-4 / 5.4(d)-2 — "How does the contractor evaluate the health risks presented by use, transport and disposal of chemicals?"

	Requested Evidence
	Appropriate SWDA Likely Chemicals MSDSs & SHOC Cards, endorsed by MD

	Assigned To
	Miracle Maduforo (Project Manager — Field Supervisor)

	Document Date
	06 August 2026



This register lists the chemicals/substances likely encountered on SWDA's tank-cleaning campaigns, drawn directly from the hazards already identified in Attachment 1 (JHSA) of the SWDA – RAEC HSE Plan, together with an MSDS summary and a Safe Handling of Chemicals (SHOC) Card for the highest-volume substance.
1.0  Likely Chemicals Register — MSDS Summary
	Chemical / Substance
	Hazard Class
	Key Health/Safety Hazards
	Required PPE
	Storage / First Aid

	Crude Oil / Gas Oil (Tank Cleaning Diluent)
	Flammable Liquid; Irritant; Suspected Carcinogen (long-term exposure)
	Skin/eye irritation; inhalation of vapours; flammability near ignition sources
	Chemical-resistant gloves, coveralls, safety glasses/goggles; ATEX equipment when handling
	Bunded storage away from ignition sources; eye wash if splashed; remove contaminated clothing

	Detergent (Tank Cleaning Agent)
	Irritant
	Skin/eye irritation on contact
	Gloves, safety glasses, coveralls for routine handling
	Store per manufacturer SDS; flush with water if contact occurs

	Nitrogen (N₂) — Tank Inerting / Purging
	Asphyxiant (simple, non-toxic but displaces oxygen)
	Asphyxiation risk in confined/poorly-ventilated spaces; no odour warning
	4-Gas Detector (O₂ monitoring), SCBA/Escape Set for CSE work under nitrogen atmosphere
	Cylinders/lines secured and leak-checked; evacuate immediately on low-O₂ alarm; move to fresh air

	Hydrogen Sulfide (H₂S) — Potential Process Residual
	Toxic Gas; Asphyxiant
	Fatal at high concentration; odour fatigue at low levels
	Personal H₂S monitors (mandatory), Breathing Apparatus (SCBA) on alarm
	Fixed H₂S monitors/alarms at work area; evacuate on activation; move casualty to fresh air, administer O₂ if trained


Full manufacturer Safety Data Sheets (SDS) for each substance are held in SWDA's Chemical Inventory file at the Lagos base office and site HSE offices, and are available to Renaissance/RAEC on request.
2.0  Sample SHOC (Safe Handling of Chemicals) Card
	Chemical
	Crude Oil / Gas Oil — Tank Cleaning Diluent

	Used For
	Automatic Tank Cleaning (ATC) dilution/transfer during tank-cleaning operations

	Physical Form
	Liquid — flammable

	Primary Hazards
	Flammable; skin/eye irritant; harmful if inhaled in vapour form; environmental hazard if spilled

	Required PPE
	Chemical-resistant gloves, coveralls, safety glasses, ATEX-rated equipment where sparks/static are possible

	Handling Precautions
	Handle only under Permit to Work; use ATEX pump for transfer; bonded hosing; cordon off works area; no ignition sources nearby; O₂/LEL monitoring where entry is required

	Storage
	Bunded storage area; away from ignition sources and incompatible materials; SDS available at point of storage

	Spill Response
	Use Oil Spill Kit immediately; contain with absorbent material; do not wash into drains; report per Environmental Policy

	First Aid — Skin Contact
	Remove contaminated clothing; wash affected area thoroughly with soap and water

	First Aid — Eye Contact
	Flush immediately with eyewash for at least 15 minutes; seek medical attention

	First Aid — Inhalation
	Move to fresh air immediately; seek medical attention if symptoms persist

	Emergency Contact
	Site HSE Officer; SWDA Emergency Response Contacts (see Section 5.1(g) Safety & Control Systems pack)


3.0  MD Endorsement
I, Gliffeth Wonuigwe, Group CEO / Managing Director of South West Design Africa Limited (SWDA), endorse the Likely Chemicals Register, MSDS Summary and SHOC Card set out above as accurate for SWDA's tank-cleaning operations.
SIGNED: ______________________________
Gliffeth Wonuigwe — Group CEO / Managing Director, SWDA Limited
Date: 06 August 2026
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