SPILL EMERGENCY RESPONSE FLOWCHART

Spill Identifier, shut in spill outlet if possible


Informs Supervisor/DSV


Spill Team Activated by  Sup/DSV





Water Qty < 1bbl
Apply Absorbent boom Skim into drum and dispose as client Management plan Clean with absorbent sheet/roll
Document incident

Clean Up Procedure Initiated
Spill Location Deck/Top Barge
Qty < 1bbl
Contain with absorbent pillows
Skim into dedicated drum Clean area with dedicated drier. E.g Bara clean
Mop surface with roll/sheet





Land Qty < 2bbl
Encircle spill with earth ring
Skim into drum Dispose spill as per client waste management plan Apply absorbent sheet or
roll to area

DSV activates spill containment team

Team deploys spill control equipment
Skim into drum in boat lean with absorbent sheet/roll Rig Deck/Top Barge Qty > 1bbl
Deploy spill control equipment to contain spread


                Land Qty > 2bbl
Make trenches/pit aroundspill area
Skim into drum evacuate with vacuum truck to flow
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