EQUIPMENT PREMOBILIZATION STATUS
	S/N
	EQUIPMENT DESCRIPTION
	DETAILS
	PRESENT LOCATION
	STATUS

	1. 
	GENERATOR I
	
	Rig 101, Escravos
	

	2. 
	GENERATOR II
	
	Rig 101, Escravos
	

	3. 
	RAM TYPE BOP
	11” x 5000psi x R53
	Michelin 
	Ok but 3⅛" weco flange for the upper ram was taken to Chevron choke manifold. Will need function testing.

	4. 
	ANNULA BOP
	11” x 5000psi x R53
	Waterfront
	Damaged element. Also needs to be panted and function tested.

	5. 
	ACCUMULATOR UNIT
	12bottles 
	Waterfront
	Bottles needs to be painted, cylinder pressure gauged, gauges recalibrated and total overhauling needed.

	6. 
	WORK WINDOW
	
	Michelin 
	Ok but mats needed to replace old mats. One of the Counterbalance gauges to be changed.

	7. 
	HOSE BASKET
	
	Michelin
	Ok but needs painting

	8. 
	STATIONARY BASKET 
	
	Michelin
	Ok

	9. 
	HYDRAULIC JACK
	
	Michelin
	Ok. Filter needs to be changed.

	10.  
	ROTARY 

	
	Michelin
	ok

	11. 
	ANCHOR BLOCKS
	
	Rig 101, Escravos
	

	12. 
	TRAVELLER SLIP
	Hydra Slip
	Michelin 
	Slip needs proper servicing and painting.

	13. 
	STATIONARY SLIP
	Cavin Slip w/dies
	Michelin
	Ok. Backup needs arm.

	14. 
	LAY DOWN WINCH
	
	Michelin
	Ok, but Roller is bad and laydown belt (minimum of 1-ton) needed also.

	15. 
	GIN POLE 
	
	Michelin
	Rigged up. Pin needed and Pump on scoping line malfunctioning.

	16. 
	TONG POLE
	
	Michelin
	ok

	17. 
	Upper LADDERS
	
	Michelin
	Rigged up. Needs to be expanded. 

	18. 
	WORK WINDOW-TO-ACCESS WINDOW LADDER
	
	Water front
	ok

	19. 
	LOWER LADDER (TO ACCESS WINDOW)
	
	Water front
	ok

	20. 
	STAND PIPE
	
	Water front
	Chicksan + swivel taken to Obeakpu. Replacement needed + pressure testing.

	21. `
	ACCUMULATOR REMOTE CONTROL PANEL
	
	Waterfront
	Needs overhauling & painting.

	22. 
	PERSONNEL BASKET 
	TNC 63TB
	Water front
	Needs to be painted.

	23. 
	TEST PUMP (equipment)
	
	Water front
	Non-functional

	24. 
	POWER PACK I  
	TN/PP-A2
(SN: 6TB17953, 420 hp)
	Water front
	Ok but needs to be re-function tested.

	25. 
	POWER PACK II
	TN/HWO/002
	Michelin
	Pump failure

	26. 
	TRIP TANK
	33bbls
	Water front
	Needs finishing in the inside and recalibration.

	27. 
	FLOW BACK TANK
	90bbls
	Obeakpu
	One agitator motor was faulty.

	28. 
	MUD PUMP I (AUTOMATIC)
	
	Obeakpu
	

	29. 
	MUD PUMP II (MANUAL)
	TN PU PM 02
	Michelin
	Clutch paddle damaged.

	30. 
	PUMP FLUID END I
	
	Obeakpu
	

	31. 
	PUMP FLUID END II
	TN PU-PE-02
	Michelin
	Needs overhauling. Valve sitting assy. needs to be changed/replaced.

	32. 
	AIR COMPRESSOR I (MANUAL)
	
	Not sighted 
	

	33. 
	AIR COMPRESSOR II (ELECTRIC)
	
	None
	

	34. 
	DIESEL TANK
	2700 ltrs
	Water front
	Body needs to be painted.

	35. 
	DIESEL TANK II
	8520 ltrs
	Water front
	Body needs to be painted.

	36. 
	CHOKE MANIFOLD
	13 valves
	Water front
	Ok but Body needs to be painted.

	37. 
	KILL MANIFOLD
	
	Obeakpu
	Ok but without check valve.

	38. 
	LOW PRESSURE MANIFOLD
	12 valves
	Water front
	Ok but Body needs to be painted.

	39. 
	DOG HOUSE 
	20ft
	Water front
	Ok but body needs to be painted.

	40. 
	MATERIAL STORE
	20ft
	Water front
	Ok but body needs to be painted + 2hp AC

	41. 
	PIPE RACKS
	4 pcs
	Water front
	ok

	42. 
	MEDIC/ELECTRICIAN CARAVAN
	
	Michelin
	Doors, windows and floor needs maintenance. AC also needed

	43. 
	FIELD ENGINEER/QHSE CARAVAN
	AC  needs servicing
	Water front
	Windows, doors and floor require thorough works. AC’s and office chairs + tables also needed.

	44. 
	SUPERVISOR’S/DSV CARAVAN
	
	Water front
	Doors, windows and floor need maintenance.

	45. 
	MUD TANK I (500BBLS)
	500 bbls
	Water front
	Inside needs finishing and manhole to be closed.

	46. 
	MUD TANK II (300BBLS)
	300 bbls
	Water front
	

	47. 
	MUD TANK III (300BBLS)
	300 bbls
	Water front
	

	48. 
	MUD TANK (extra mud tank during Agip operation)
	300 bbls
	Water front
	To be backloaded to base

	49. 
	PUMPING BASKET WITH ACCESSORIES
	
	Water front
	Basket contains the following:
1. 4pcs 3⅛" Blind Flange
2. 1 pc 3⅛" x 4" Weco Flange
3. 2pcs 2" x 10’ Chicksan
4. 6pcs 2" female Weco
5. 1pc 2-1/16" Weco Flange
6. 2pcs 2" Relief Valve
And basket needs painting.

	1. 
	CENTRIFUGAL PUMP 1 
	
	Obeakpu
	

	2. 
	CENTRIFUGAL PUMP 2
	
	Obeakpu
	

	3. 
	ELECTRIC CENTRIFUGAL PUMP
	CP (MCM, SN: 25905, mode:  250x series)
	Water front
	

	4. 
	ELECTRIC PANNEL
	
	Michelin
	ok

	5. 
	CYLINDER BASKET
	
	Waterfront
	Body needs painting.

	6. 
	SLING RACK
	
	Water front
	Require painting.

	7. 
	Y-T elevator
	
	Water front
	Needs to be taken to Workstring for thorough maintenance.

	8. 
	CHOKE REMOTE PANEL (SWACO DETECTION CONTROL) S/N: 1427
	
	Water front
	Panel require over hauling and painting.

	9. 
	WELDERS TOOL BOX
	
	Water front
	Ok

	10. 
	BASKET W/11” X 5K X R53 SPOOL
	
	Water front
	Require painting

	11. 
	WELDING MACHINE
	N15130
	
	Needs to be backloaded to Fabrication Dept.

	12. 
	HYDRIL ANNULAR BOP 
	(GK-10-1500-31400)
	Water front (On a travelling skid)
	Bad element. To be backloaded to Michelin for thorough maintenance.

	13. 
	ADAPTER FLANGE
	5K x 3K
	Water front
	Ok

	14. 
	LOW PRESSURE HOSE BASKET

	
	Water front
	Contains: 
1. 4” x 150psi x 9pcs hose 
2. 6” x 150psi x 2pcs hose

	15. 
	EMPTY GAS CYLINDER
	3pcs 
	Water front
	

	16. 
	AIR MANIFOLD
	1pc
	Water front
	

	17. 
	EYE WASH
	
	Water front
	Ok but inside needs to be treated.

	18. 
	WEAR BUSHING 
	
	Water front
	

	19. 
	CROSS OVER BOX
	
	Water front
	



